# Required Components

|  |  |
| --- | --- |
| Both halves of the device, laid out and numbered | **BOM**   1. Aid-top 2. Aid-bottom |

# Required Tools

* Soldering iron

# Required Personal Protective Equipment (PPE)

* Eye protection

# Assembly Instructions

## Step 1

Align the two halves of the device and run a soldering iron around the seam shown with the red dotted line to ‘weld’ the two halves together. This should be done in a well-ventilated room. Alternatively, the two halves of the device could be glued together.

